|  |  |  |  |
| --- | --- | --- | --- |
| REVISION HISTORY | | | CPLD CONTROL TOOL SPECIFICATION |
| Rev. | Date | Description | |
| Page/Article | Summary |
| 1.0 | Sep 02, 2020 | ⎯ | New creation |
| 1.3 | Sep 25, 2020 | 1.4 | Remove half-powered USB restriction, already implemented a work-around for it  Add udev rule part |
| 4.3.1 | Libconfuse: add method to fix issue config.guess |
| 5 | Update display sample of version 1.3 |
| 1.4 | Oct 30, 2020 | 1.4 | Add notice about the CPLD firmware version for each board |
| 4.1 | Remove file CPLD\_register.txt in folder structure (this info is now in source code) |
| 4.3.2 | Remove the restriction of the stored place of CPLD\_register.txt file. |
| 1.5 | Dec 02, 2020 | ⎯ | Add board V3M Starter Kit |
| 3.6 | Add command CPLD write non-volatile |
| 5 | Add new sample log |
| 1.6 | July 16, 2021 | ⎯ | Modify the protocol for V3MSK to SMI |
| 1.7 | Aug 04, 2020 | ⎯ | Add board S4 Spider |